**The organ specification**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Great cc-g’’’ | Swell cc-g’’’ | Pedal ccc-f’ | Couplers | Mixture |
| Open Diapason 8 | Lieblich Bourdon 16 (to tenor C only) | Bourdon 16 | Swell to Great | 1-25 15.19.22  26-25 8.12.15 |
| Wald Flute 8 | Open Diapason 8 | spare stop | Swell to Pedal |  |
| Dulciana 8 | Stopped Diapason 8 |  | Great to Pedal |  |
| Principal 4 | Gamba 8 |  |  |  |
| Lieblich Flute 4 | Voix Celeste 8 |  |  |  |
| Fifteenth 2 | Principal 4 |  |  |  |
| Clarinet 8 | Mixture iii |  |  |  |
|  | Horn 8 |  |  |  |
|  | Oboe 8 |  |  |  |

3 composition pedals to Great

3 composition pedals to Swell

Latch-down Swell lever

One double-rise reservoir (no manual supply)

Wind Pessure: 76mm